UNIT AMENDMENTS
A- WORKTOP
· Light needs taking in by 10mm to allow for t-trim cut
· Back has rounded corners, these need to be square, look at finish of rear of cabinet
· Track recess needs extending to front of cabinet to panel C (or beyond)
· Check track measurement on drawing 12mm ? ( last cut at 10mm)
· Smev cut-out needs reducing 
· Smev corners need to be amended to allow for fixing.
· Smev cut-out needs centering 
· Discuss R/H & L/H options (possibly invert)

B- BASE
· Track needs extending to panel C (or beyond)
· Possible rounded edges to rear of cabinet?

C- CUPBOARD FASCIA PANEL
· Width needs reducing to 500mm
· Apertures need to be centered in relation to concealment of one side into corner profile

D- SIDE PANEL (RIGHT)
· Needs reducing ( no need for scribing)

E- BACK PANEL
· OK

F- SIDE PANEL (LEFT)
· Needs increasing to 150mm

G- INNER SIDE PANEL
· Needs increasing to 80mm

H- BACK PANEL
· Needs increasing to 962mm

I- SHELF
· Needs to be 962mm x 373mm
· Needs an allowance to account for inner corner profile.
· Needs curve to follow Tambour door contour

J- BOTTOM CENTRE DIVIDE
· Depth 373mm
· Height 440mm




